{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["文化建设","Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"文化建设","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"merged":[[1,0,1,7],[2,0,2,7],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[3,7,4,7]],"flags":["formulas_cached_only"]}
[]
["珠海市卫生学校2017校园文化建设采购项目"]
["内容及要求"]
["序号","工程项目 ","单位","数量","规格","综合单价","小计","备注"]
[]
[1,"9楼宣传栏","个",2,"120cmX240cm"," "," ","镀锌板、铝合型材\n氟碳喷涂工艺\n设计排版钢化玻璃PC耐力板\n液压开启、宣传栏内容包含设计\n安装人工及辅材"]
[2,"9楼会议室背景墙                         ","M2",20.8,"690cmX300cm"," "," ","1、木制品做框架 2、护墙板对墙做防水处理，衬底木档 3、面板不论漆料，油漆先做色板 4、采用贴面材料时（平整、牢固、不脱胶、不漏胶）5、注意钉眼之间的距离不大于10CM钉眼间距均匀，不打乱钉"]
[3,"10楼宣传栏","个",2,"120cmX240cm"," "," ","镀锌板、铝合型材\n氟碳喷涂工艺\n设计排版钢化玻璃PC耐力板\n液压开启、宣传栏内容包含设计\n安装人工及辅材"]
[4,"10楼会议室挂画","个",16,"60cmX90cm"," "," ","镀锌板、铝合型材\n电镀喷砂工艺\n设计排版钢化玻璃PC耐力板\n宣传栏内容包含设计\n安装人工及辅材"]
[5,"10楼党建室宣传图","个",1,"120cmX240cm"," "," ","高级相框材料\n5MMPVC板喷绘处理\n宣传栏内容包含设计\n安装人工及辅材"]
[6,"9楼、10楼主题文化宣传图（走廊区、护士站实验区）","个",81,"40cmX60cm"," "," ","镀锌板、铝合型材\n电镀喷砂工艺\n设计排版钢化玻璃PC耐力板\n宣传栏内容包含设计\n安装人工及辅材"]
[7,"班徽","套",32,"40cmX40cm"," "," ","2张5MM进口亚克力\n4套304实心广告螺丝\n设计排版\n1张相纸过亚膜\n安装人工及辅材"]
[8,"班训","套",32,"40cmX200cm"," "," ","9MM进口高密度软木板;环保优质麻布;进口橡木边框;5MM环保底板;6MMPVC高密度板;高清背胶;设计排版;安装人工及辅材"]
[9,"学生公约","套",32,"80cmX120cm"," "," ","2张5MM进口亚克力\n4套304实心广告螺丝\n设计排版\n1张相纸过亚膜\n安装人工及辅材"]
[10,"社会主义核心价值观","套",32,"80cmX120cm"," "," ","2张5MM进口亚克力\n4套304实心广告螺丝\n设计排版\n1张相纸过亚膜\n安装人工及辅材"]
[11,"公示栏","套",32,"80cmX120cm"," "," ","9MM进口高密度软木板;环保优质麻布;进口橡木边框;5MM环保底板;6MMPVC高密度板;高清背胶;设计排版;安装人工及辅材"]
[12,"荣誉栏","套",32,"40cmX200cm"," "," ","9MM进口高密度软木板;环保优质麻布;进口橡木边框;5MM环保底板;6MMPVC高密度板;高清背胶;设计排版;安装人工及辅材"]
[13,"支部园地","套",32,"80cmX120cm"," "," ","9MM进口高密度软木板;环保优质麻布;进口橡木边框;5MM环保底板;6MMPVC高密度板;高清背胶;设计排版;安装人工及辅材"]
[14,"班级文化栏","套",32,"120cmX240cm","  "," ","9MM进口高密度软木板;环保优质麻布;进口橡木边框;5MM环保底板;6MMPVC高密度板;高清背胶;设计排版;安装人工及辅材"]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}